The Following for a size **WP**-**17** **air cooled torch**:

• 1 Pack tungsten (2% ceriated or Lanthanated ) size .040, 1/16, 3/32, and 1/8”

* 2- Collet for each size tungsten
* 2- Collet Body or each size tungsten
* 2- Gas Lens or each size tungsten

• Tig cup sizes 4 - 12 for the collet and collet body

* Tig cup sizes 4 - 12 for the collet and Gas Lens
* Welding helmet
* Tig torch Stand
* Mini Bolt Cutters
* Tig gloves
* Plano Tackle box for torch parts and tungsten
* USB Storage device